Getting started

Note: the map data is due to revision in fall 2018. Check this page for any updates.

How to add Anglova Scenario to SDT3D

Download and extract sdt3d package

Extract worldwind.jar package maintaining hierarchy

Edit file config/worldwind.layers.xml by adding line along similar lines (e.g. after OpenStreetMap) <Layer href="config/Earth/AnglovaScenario.xml" actuate="onRequest"/>

Copy AnglovaScenario.xml into config/Earth/ folder.

Update / add above files into worldwind.jar (or repack whole hierarchy)

Start sdt3d

How to add Anglova Scenario to GIS software as WMS layers

WMS service endpoint is at https://wms.anglova.net/wms. The Service is running mapproxy version 1.9, so it supports WMS 1.0.0, 1.1.1, and 1.3.0. There are two layers available:

ist124 that provides the Anglova Scenario mapping information

osm provides standard OpenStreetMap rendering

For previous instructions the domain name will change from cnict.org to anglova.net in AnglovaScenario.xml. The older URL still works identically.

How to use tile map service

Map is also available as standard tile map service. The URL follows standard format https://tile.site.example/Z/X/Y.png where tile.site.example is tile.anglova.net. If you have a software that uses OpenStreetMap tiles, just replace tile.openstreetmap.org with tile.anglova.net.

Map preview is available at https://tile.anglova.net.