SCB under jamming

Following data files include computed topology in a special case when the company is jammed from quite far away with free line of sight. The pathloss threshod is reduced with value 5 - 25 dB.

139-5 dB

139-10 dB

139-15 dB

139-20 dB

139-25 dB

Connectivity graphs per company

Company 1

Company 2

Company 3

Company 4

Company 5

Company 6