Synchronized Cooperative Broadcasting

The Synchronized Cooperative Broadcast (SCB) waveform was designed to transport primarily broadcast traffic within multi-hop mobile networks.

Precomputed SCB topology that mimics a static SCB network and allows us to fully model SCB’s cooperative effects. In this method we calculate the sum of receive power from transmitting nodes and compare that to a pathloss threshold (139 dB), to determine the set of nodes that are reachable, via multi-hop, from a given source node.

Data files

Pathloss threshold 139 dB

Different scenarios

Pathloss in jammed