Synchronized Cooperative Broadcasting

The Synchronized Cooperative Broadcast (SCB) waveform was designed to transport primarily broadcast traffic within multi-hop mobile networks.

Precomputed SCB topology that mimics a static SCB network and allows us to fully model SCB’s cooperative effects. In this method we calculate the sum of receive power from transmitting nodes and compare that to a pathloss threshold (139 dB), to determine the set of nodes that are reachable, via multi-hop, from a given source node.

Data files

Pathloss threshold 139 dB

Following data files include computed topology in a special case when the company is jammed from quite far away with free line of sight. The pathloss threshod is reduced with value 5 - 25 dB.

5 dB

10 dB

15 dB

20 dB

25 dB

Connectivity graphs per company

Company 1

Company 2

Company 3

Company 4

Company 5

Company 6